**MI-004 approval for WATERFLUX and OPTIFLUX electromagnetic flowmeters**

* To be used as thermal energy meters as part of a heat metering system
* MI-004 calibration can be realized through either Module D or Module F

**Text:**

Duisburg, March 12, 2019: Electromagnetic flowmeters WATERFLUX 3300, WATERFLUX 3070 and OPTIFLUX 4300 are now available with approval according to MID 2014/32/EU annex VI MI-004 for thermal energy meters. Together with ultrasonic flowmeter OPTISONIC 3400 District Heating, they form KROHNEs flow meter portfolio to be used as part of a heat metering system. Typical applications include custody transfer (fiscal metering) in district heating networks, commercial and industrial heat metering or general energy and utility applications in combined heat and electricity generation.

The MI-004 calibration can be realized through either Module D or Module F. With Module D, the calibration is performed by KROHNE Altometer in Dordrecht, The Netherlands, which has been accredited by the NMI to perform MI-004 calibrations. With Module F, the calibration is performed by a notified body specifically requested by the customer, e.g. MID-Cert in Germany.

About KROHNE:

KROHNE is a full-service provider for process measuring technology for the measurement of flow, mass flow, level, pressure and temperature as well as analytical tasks. Founded in 1921 and headquartered in Duisburg, Germany, the company employs over 3,700 people all over the world and is present on all continents. KROHNE stands for innovation and maximum product quality and is one of the market leaders in industrial process measuring technology.

**Picture:**



**Caption:** WATERFLUX and OPTIFLUX electromagnetic flowmeters now available with MI-004 approval

Issued by:

KROHNE Messtechnik GmbH

Ludwig-Krohne-Str. 5

47058 Duisburg

[www.krohne.com](http://www.krohne.com)

Press contact:

Jörg Holtmann, PR Manager

Tel: +49 203 301 4511

[j.holtmann@krohne.com](mailto:j.holtmann@krohne.com?subject=ISA%20Messe-Award%20für%20UFM%203030)